Press release from PEAK-System Technik, Darmstadt, Germany, January 2014
========================================================================

CAN to WLAN Gateways in a plastic housing with a flange

PEAK-System complements its new gateway product family by two other WLAN-enabled devices. The PCAN Wireless Gateways facilitate the connection of CAN busses over WLAN. For this, CAN frames are wrapped in TCP or UDP message packages and forwarded from one device to another over the IP network. Configuration of the devices is provided by a convenient web interface.

The PCAN Wireless Gateways are supplied in a plastic housing with a flange and are available in 2 versions; one with two 9-pin D-Sub connectors and the other with a 12-pin Tyco automotive connector. Built in are two High-speed CAN channels with a bit rate of up to 1 Mbit/s. The WLAN interface supports IEEE 802.11 b/g and establishes its connection via an internal chip antenna. Thanks to its extended operating temperature range of -40 to 85 °C (-40 to 185 °F) the PCAN-Wireless Gateway is suitable for use in industrial and automotive environments.


Contact:
PEAK-System Technik GmbH
Otto-Roehm-Strasse 69
64293 Darmstadt
Germany

Phone: +49 (0)6151-8173-20
Fax:   +49 (0)6151-8173-29

E-mail: info@peak-system.com
Web:    www.peak-system.com
