Press Release by PEAK-System Technik GmbH, January 2011
-------------------------------------------------------

New product: CAN repeater with galvanic isolation

The new PCAN-Repeater by PEAK-System connects two High-speed CAN busses with a galvanic isolation up to 5 kV. Both CAN channels as well as the CAN channels and the voltage supply are decoupled against each other. CAN messages are forwarded 1:1 between both CAN channels, also in a single direction if required. LEDs indicate the current bus status. The module is designed for use in industrial environments, with features like the enhanced temperature range of -40 to +85 °C and the top-hat rail mounting.

Contact:
PEAK-System Technik GmbH
Otto-Roehm-Strasse 69
64293 Darmstadt
Germany

Phone:  +49 (0)6151 8173-20
Fax:    +49 (0)6151 8173-29
E-mail: info@peak-system.com
Web:    www.peak-system.com
